# Software Information
display_name = "Wenquxing (WQXEmu)"
authors = "Aloys"
supported_extensions = ""
corename = "wqxemu"
categories = "Emulator"
license = "GPL-3.0-or-later"
permissions = ""
display_version = "0.1.0"

# Hardware Information
manufacturer = "Wenquxing"
systemname = "Wenquxing"
systemid = "wenquxing"

# Libretro Features
database = "Wenquxing"
supports_no_game = "true"
savestate = "true"
cheats = "false"
input_descriptors = "true"
memory_descriptors = "false"
libretro_saves = "true"
core_options = "true"
load_subsystem = "false"
hw_render = "false"
needs_fullpath = "false"
disk_control = "false"
is_experimental = "false"

# Firmware / BIOS
firmware_count = 12
firmware0_desc = "NC1020 obj_lu.bin (System ROM)"
firmware0_path = "WQXEmu/nc1020/obj_lu.bin"
firmware0_opt = "true"
firmware1_desc = "NC1020 nc1020.fls (NOR Flash)"
firmware1_path = "WQXEmu/nc1020/nc1020.fls"
firmware1_opt = "true"
firmware2_desc = "PC1000 pc1000.rom (System ROM)"
firmware2_path = "WQXEmu/pc1000/pc1000.rom"
firmware2_opt = "true"
firmware3_desc = "PC1000 pc1000.fls (NOR Flash)"
firmware3_path = "WQXEmu/pc1000/pc1000.fls"
firmware3_opt = "true"
firmware4_desc = "CC800 obj.bin (System ROM)"
firmware4_path = "WQXEmu/cc800/obj.bin"
firmware4_opt = "true"
firmware5_desc = "CC800 cc800.fls (NOR Flash)"
firmware5_path = "WQXEmu/cc800/cc800.fls"
firmware5_opt = "true"
firmware6_desc = "NC2000 nc2000.nor (NOR Flash)"
firmware6_path = "WQXEmu/nc2000/nc2000.nor"
firmware6_opt = "true"
firmware7_desc = "NC2000 nc2000.nand (NAND Flash)"
firmware7_path = "WQXEmu/nc2000/nc2000.nand"
firmware7_opt = "true"
firmware8_desc = "NC2000 nc2000.nand0 (First NAND Plane)"
firmware8_path = "WQXEmu/nc2000/nc2000.nand0"
firmware8_opt = "true"
firmware9_desc = "NC3000 nc3000.nor (NOR Flash)"
firmware9_path = "WQXEmu/nc3000/nc3000.nor"
firmware9_opt = "true"
firmware10_desc = "NC3000 nc3000.nand (NAND Flash)"
firmware10_path = "WQXEmu/nc3000/nc3000.nand"
firmware10_opt = "true"
firmware11_desc = "NC3000 nc3000.nand0 (Optional First NAND Plane)"
firmware11_path = "WQXEmu/nc3000/nc3000.nand0"
firmware11_opt = "true"

notes = "(!) Firmware entries are conditionally required for the model selected in Core Options.|(!) NC3000 nc3000.nand0 is optional; all other files for the selected model are required."
description = "WQXEmu emulates NC1020, PC1000, CC800, NC2000, and NC3000 Wenquxing electronic dictionaries. Select a model in Core Options and start the core without content. Original hardware firmware must be placed under the frontend system directory in WQXEmu/<model>/."
